Гуманитарный проект отдела по образованию Барановичского райисполкома Брестской области ищет спонсоров
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Цель проекта: создание на базе детского оздоровительного лагеря «Дружба» оптимальных условий для укрепления здоровья, полноценного отдыха детей – инвалидов, детей с особенностями психофизического развития (далее ОПФР); оказание им помощи в социальной адаптации и реализации их личного потенциала
1. Наименование проекта: модернизация детского оздоровительного лагеря «Дружба»
2. Срок реализации проекта: 24 месяцa
3. Организация - заявитель, предлагающая проект: отдел по образованию Барановичского райисполкома
4. Цель проекта: создание на базе детского оздоровительного лагеря «Дружба» оптимальных условий для укрепления здоровья, полноценного отдыха детей – инвалидов, детей с особенностями психофизического развития (далее ОПФР); оказание им помощи в социальной адаптации и реализации их личного потенциала
5. Задачи, планируемые к выполнению в рамках реализации проекта:
· модернизация системы отопления (кварцевые обогреватели);
· замена инженерных коммуникаций, санитарно-технического и технологического оборудования (электроплиты, пищеварочные котлы, холодильное оборудование);
· установка пандусов, электроподъемного оборудования и грязезащитного покрытия (для инвалидов-колясочников);
· внутренние отделочные работы;
· ремонт кровли, установка двускатной крыши;
· работы по ремонту фасада зданий, укладка тротуарной плитки;
· замена оконных и дверных блоков, напольного покрытия;
· оборудование уличных игровых площадок;
· оборудование сенсорной комнаты, приобретение костюмов и реквизита для игр (для клоунов-волонтеров);
· оборудование бытовых комнат в корпусах.
6. Целевая группа: дети в возрасте 6-18 лет, в т.ч. дети – инвалиды, дети с особенностями психофизического развития
7. Краткое описание мероприятий в рамках проекта:
-Капитальный ремонт с элементами модернизации административных и спальных корпусов. 

-Создание сенсорно-динамического зала и комплектация групп специальным оборудованием для занятий по сенсорной интеграции:

мат напольный, «мягкое бревно», веревка альпинистская, «мягкий тоннель», платформа качающаяся, сенсорный гамак, «мягкие качели-лента», одеяло с утяжелителем, подушка,  жилет с утяжелителем, мяч-скакун, равновес, набор мягких строительных блоков, набор мешочков-утяжелителей, балансир, батут, бочка, бревно,  фитбол;  наклонная поверхность, мягкий геометрический модуль, роликовые доски (квадратные подставки на колесиках), сиденье-тарелка, кресла-мешки, парашют;

модернизация сенсорной среды - оформление «Сенсорных копилок» (стеллажи, контейнеры разных размеров, материла для наполнения сенсорных коробок);

семинары, тренинги, конференции;

комплекс практических мероприятий (мастер-классы, семинар-практикум «Ребенок и сенсорная интеграция», интенсив «Ярмарка вкуса»);

повышение профессиональной компетентности специалистов (образовательные курсы для педагогов).
	8. Общий объем финансирования (в долларах
	США): 320 000

	Источник финансирования
	Объем финансирования (в долларах США)

	Средства донора
	320 000

	Софинансирование
	-

	9. Место реализации проекта (область/район, город): Брестская область, Барановичский район, дер. Переносины

	10. Контактное лицо:
	

	О.В.Воляк, начальник отдела по образованию Барановичского райисполкома, телефон 8(0163)64-06-15, e-mail: roo@bar-roo-edu.brest.by.
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Будем рады сотрудничеству!

1. Введение
Гуманитарный проект «Модернизация детского оздоровительного лагеря «Дружба» по адресу: Брестская область, Барановичский район, дер. Переносины выполнен в целях реализации Комплекса мер по привлечению иностранной безвозмездной помощи в Республику Беларусь до 2020 года и других исходных данных.
Благоустраиваемая площадка расположена на территории детского оздоровительного лагеря «Дружба» размещенного в лесу, в 25 км от г. Барановичи, 4 км от ж.д. станции Полонка. Территорию лагеря окружают хвойные и смешанные леса, она не имеет непосредственной границы с транспортными коммуникациями. На территории лагеря находится радоновый источник, местонахождение которого планируется облагородить, установить вокруг него беседку и использовать его по назначению медицинского работника для соответствующих категорий детей, находящихся на оздоровлении в лагере. 
Проектом модернизации предусматривается:

- модернизация системы отопления;
-замена инженерных коммуникаций, санитарно-технического и технологического оборудования (электроплиты, пищеварочные котлы, холодильное оборудование);

- установка пандусов, электроподъемного оборудования и грязезащитного покрытия (для инвалидов-колясочников);

- внутренние отделочные работы;

- ремонт кровли, установка двускатной крыши;

- работы по ремонту фасада зданий, укладка тротуарной плитки (1560 м2);

- замена оконных (66,5 м2) и дверных блоков (45 м2), напольного покрытия (190 м2);

- переустройство спортивно-игровой зоны лагеря с модернизацией площадок и размещением спортивного и игрового оборудования;
- оборудование сенсорной комнаты, приобретение костюмов и реквизита для игр (для клоунов-волонтеров);

- оборудование бытовых комнат в корпусах;

- устройство новых пешеходных связей на территории лагеря, велосипедных дорожек, создание экологических троп на территории леса, окружающего ОЛ «Дружба».
2. Описание решений по благоустройству территории

Благоустройством предусмотрено:

- установка пандусов, электроподъемного оборудования и грязезащитного покрытия (для инвалидов-колясочников);
- устройство пешеходных дорожек, велосипедных дорожек, газонов,  скамеек и беседок;
- покрытие дорожек из мелкоразмерной бетонной плитки (100 м2) с установкой тротуарного бетонного борта;

 - переустройство спортивно-игровой зоны лагеря с модернизацией площадок и размещением спортивного и игрового оборудования.

3. Описание решений по функциональному зонированию
Рис.1. Схема модернизации территории оздоровительного лагеря «Дружба».

Условные обозначения зон:

1 - входная группа с распределительной площадкой

2 - зона общественных собраний

3 - хозяйственная зона

4 - детская развлекательная зона

5 - спортивная зона

6 - зона отрядов

7 - зона тихого отдыха
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Площадка в плане представляет собой сложную форму. Территория имеет четкое зонирование.
У главного входа на территорию детского лагеря проектом предусмотрено размещение площадки для распределения отдыхающих по отрядам, приема гостей. Также в этой зоне предусмотрено размещение гостевого домика-сторожки. 

Зона общественных собраний примыкает к входной зоне для удобного пользования как отдыхающими, так и гостями оздоровительного лагеря. В зоне общественных собраний предусмотрено размещение сцены и танцевальной площадки, на которой помимо развлекательных мероприятий также можно устраивать и общественные собрания. В этой зоне надо создать условия для нахождения инвалидов – колясочников.
В центре территории оздоровительного лагеря, между жилыми корпусами и столовой предусмотрено размещение уличной игровой площадки с созданием условий нахождения на ней также и инвалидов-колясочников. На игровой площадке планируется установка детских качалок, горок, песочниц и т.д. 
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В зоне тихого отдыха,  между деревьями предусмотрено размещение 8 беседок с навесами вместимостью 25 человек каждая. 
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В северо-западной части участка проектом предусмотрено размещение спортивно-развлекательной зоны. Предусматривается размещение спортивных тренажеров различного назначения, а также площадки для «воркаута», батутов.
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В детской развлекательной зоне проектом предусмотрено размещение детского городка для детей 6-10 лет с установкой оборудования для игр и активного отдыха. 
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По периметру территории предусмотрено устройство велосипедной  дорожки. 
В здании медицинского блока проектом предусмотрено создание сенсорно-динамического зала и комплектация групп специальным оборудованием для занятий по сенсорной интеграции: мат напольный, «мягкое бревно», веревка альпинистская, «мягкий тоннель», платформа качающаяся, сенсорный гамак, «мягкие качели-лента», одеяло с утяжелителем,  подушка,  жилет с утяжелителем, мяч-скакун, равновес, набор мягких строительных блоков, набор мешочков-утяжелителей, балансир, батут, бочка, бревно,  фитбол;  наклонная поверхность, мягкий геометрический модуль, роликовые доски (квадратные подставки на колесиках), сиденье-тарелка, кресла-мешки, парашют; модернизация сенсорной среды - оформление «Сенсорных копилок» (стеллажи, контейнеры разных размеров, материла для наполнения сенсорных коробок).  
Для хозяйственной зоны проектом предусматривается замена инженерных коммуникаций, санитарно-технического и технологического оборудования (электроплиты, пищеварочного котла, холодильное   оборудование). Проектом благоустройства предусматривается ремонт кровли и установка двускатной крыши на здании столовой. 

Проектным решением принято произвести работы по замене оконных и дверных блоков, напольного покрытия, внутренние отделочные  работы, работы по оборудованию бытовых комнат в корпусах; модернизации системы отопления.

Проектом благоустройства предусматривается установка пандусов, электроподъемного оборудования и грязезащитного покрытия для инвалидов-колясочников.
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4. Описание решений по обеспечению условий жизнедеятельности маломобильных групп населения
Необходимо предусмотреть условия беспрепятственного и удобного передвижения маломобильных групп (МГН) по территории проектирования с учетом требований градостроительных норм к параметрам путей движения. Трассировка проектируемых пешеходных путей – короткие, спрямленные, просматриваемые на всем протяжении. Парковочные места для инвалидов расположены в непосредственной близости от объекта.  Наименьшая ширина тротуара принята 1,5 м, бортовые камни установлены без перепада высот, что обеспечивает беспрепятственное периодическое движение лиц, передвигающихся на креслах-колясках, от проездов по  тротуару  на площадки, расположенные у входа в здание. Габариты площадок позволяют выполнить свободный разворот кресла-коляски как непосредственно в месте входа в здание, так и по пути движения инвалидов-колясочников. Проектом предусматриваются дублирующие лестницы, тротуары-пандусы для инвалидов с уклоном, не превышающим 58 %. Продольный уклон пути движения, по которому возможен проезд инвалидов на креслах-колясках, принят 0,5%-5,8%. При устройстве съездов с тротуара продольный уклон увеличен до 10% на расстоянии  2,0 м от бортового дорожного камня. Поперечный уклон принят в пределах 1-25%.

Съезды с тротуаров на проезжую часть проезда выполнены с уклоном 5-10%, размер площадки перед началом съезда принят  0,8-1,5м, цвет и фактура на всем протяжении контрастируют с цветом и фактурой прилегающих поверхностей. 

Уровни пересечения путей движения по тротуару с проездами выполнены на одном уровне. Высота бортового камня в местах пересечения тротуаров с проезжей частью, а также бордюры бортовых камней вдоль эксплуатируемых газонов и озелененных площадок, примыкающих к путям пешеходного движения, установлены без перепада высот.

Для покрытия пешеходной дорожки необходимо применить плиты бетонные тротуарные мелкоштучные. Поверхность покрытия – прочная, твердая, нескользкая, толщина швов между плитками не более 10 мм, что обеспечивает беспрепятственное и удобное передвижение маломобильных групп (МГН) по пешеходной дорожке.

Humanitarian project of education department of Baranovichi district executive committee of Brest region is looking for sponsors

	
	

	1. Name of the project: Children’s summer camp “Druzhba” modernization 

	2. Project implementation period: 24 months

	3. Organization, which offers a project: Department of Education of Baranovichi District Executive Committee

	4. Project objectives: creation of optimal conditions for health promotion, recreation of children with disability, feature of psychophysical development; assistance in social adaptation and realization of their personal potential

	5. Tasks to be realized while the project implementation: 

- modernization of heating system (quartz heaters); 

- replacement of utilities, sanitary and technological equipment (electric stoves, cooking boilers, refrigeration equipment); 

- installation of ramps, electric lifting equipment and dirt-proof cover (for wheelchair users); 

- interior finishing works; 

- roof repair, installation of gable roof; 

- works on repair of a facade of buildings, paving slabs laying; 

- replacement of window and door blocks, floor covering; 

- equipment of outdoor playgrounds; 

- touch room equipment, purchase of costumes and props for games (for clowns-volunteers); 

- the household equipment of the rooms in the buildings.

	6. Task group: children at the age of 6-18, children with disabilities, feature of psychophysical development

	7. Brief description of the events within the framework of the project:  

- Capital repair with modernization of administrative buildings and dormitories.

- The creation of a sensory-dynamic room and the assembly of groups with special equipment for sensory integration classes: protection of vertical posts 1.65x0.14 m on fasteners, floor mat, “soft log”, climbing rope, “soft tunnel”, swing platform, touch hammock, “soft swing ribbon ", egg Kisling, pendalin, elastic scarf, blanket with weighting agent, pillow, vest with weighting agent, ball-horse, equilibrium, the set is soft x building blocks, a set of sacks-weighting agents, a balance weight, a trampoline, a barrel, a log, a fitball;  inclined surface, soft geometric module, roller boards (square supports on castors), seat-plate, bean bags, parachute.

modernization of the sensory environment - design of “Touch moneyboxes” (racks, containers of different sizes, materials for filling the sensor boxes).

seminars, trainings, conferences;

a set of practical activities (master classes, workshop “Child and sensory integration”, intensive “Fair of Taste”);

increasing the professional competence of the centre's specialists;

informational and educational activities (photo exhibition “We see, we feel”, informing in the media).

	8. Total funding (dollars USA): 320 000

	Source of funding
	Amount of financing 

(dollars USA)

	Contributor
	320 000

	Co-financing
	-

	9. Place of the project implementation (region/district, town): Brest region, Baranovichi district, Perenosiny village 

	10. Contact person: S.V.Ryasnyanskij, director of the children's camp "Druzhba", tel. 8(0163)63-90-53, e-mail: roo@bar-roo-edu.brest.by.




We look forward to collaborating!

1. Introduction
Humanitarian project " Modernization of children's health camp "Druzhba" at the address: Brest region, Baranovichi district, Perenosiny village was carried out in order to implement a Set of measures to attract foreign gratuitous assistance to the Republic of Belarus until 2020 and other initial data.
The landscaped area is located on the territory of the children's health camp "Druzhba" located in the forest, 25 km from the city of Baranovichi, 4 km from the railway station Polonka. The territory of the camp is surrounded by coniferous and mixed forests, it has no immediate border with transport communications. On the territory of the camp there is a radon spring, the location of which is planned to improve, install a gazebo around it and use it for the purpose of a medical worker for the relevant categories of children who are on recovery in the camp.

The modernization project provides: 
- modernization of the heating system; 
- replacement of utilities, sanitary and technological equipment (electric stoves, cooking boilers, refrigeration equipment); 
- installation of ramps, electric lifting equipment and dirt cover (for wheelchair users); 
- interior finishing works; 
- roof repair, installation of gable roof; 
- works on repair of a facade of buildings, laying of paving slabs (1560 m2); 
- replacement of window (66.5 m2) and door blocks (45 m2), flooring (190 m2);

- reconstruction of the sports and playing area of the camp with the modernization of sites and placement of sports and gaming equipment; 
- sensor room equipment, purchase of costumes and props for games (for clown volunteers); 
- equipment of household rooms in buildings; 
- the device of new pedestrian links in the camp, Bicycle paths, the creation of ecological trails in the forest surrounding the HC "Druzhba".
2. Description of solutions for landscaping
Landscaping provided: 
- installation of ramps, electric lifting equipment and dirt cover (for wheelchair users); 
- arrangement of footpaths, Bicycle paths, lawns, benches and gazebos; 
- covering tracks from a small concrete tile (100 m2) installation of concrete sidewalk board; 
- reconstruction of the sports and playing area of the camp with the modernization of sites and placement of sports and gaming equipment.

3. Description of functional zoning solutions
Figure 1. Scheme of modernization of the territory of the camp "Druzhba". 
Legend zones: 
1 - entrance lobby with control pad 
2 - public meeting area 
3 - shopping area 
4 - children's entertainment area 

5 - sports area 

6 - zone units 

7 - area for recreation
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The site in the plan is a complex shape. The territory has a clear zoning. 
At the main entrance to the territory of the children's camp, the project provides for the placement of a platform for the distribution of vacationers by units, reception of guests. There is also a gatehouse in this area. 
The public meeting area is adjacent to the entrance area for convenient use by both vacationers and guests of the health camp. In the area of public meetings, there is a stage and a dance floor, where in addition to entertainment events, public meetings can also be arranged. In this zone it is necessary to create conditions for finding wheelchair users.
In the center of the territory of the health camp, between the residential buildings and the dining room, there is a street Playground with the creation of conditions for wheelchair users. On the Playground it is planned to install children's rocking chairs, slides, sandboxes, etc.

In the quiet recreation area, between the trees there are 8 gazebos with canopies for 25 people each.
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In the north-western part of the site, the project provides for the placement of a sports and entertainment zone. It provides for the placement of sports simulators for various purposes, as well as platforms for "workout", trampolines.
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In the children's entertainment area, the project provides for the placement of a children's camp for children 6-10 years with the installation of equipment for games and outdoor activities.
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Along the perimeter of the territory there is a device of a bicycle path. In the building block, the project envisages the creation of touch-hall and the dynamic forming of groups with special equipment for the sensory integration: a floor mat, "soft log", rope climbing, "soft tunnel", the platform is oscillating, touch the hammock, "the soft swing-tape", a blanket with weighting material, a pillow, a vest with weighting material, the ball-roller, equilibrium, soft building blocks, a set of bags of weights, balance bar, trampoline, barrel, log, fitball; inclined surface, soft geometric module, roller boards (square stand on wheels), the seat-plate, bean bags, parachute; modernization of the sensory environment design "Touch piggy banks" (racks, containers of different sizes, the material for filling the touch boxes).
For the economic zone, the project provides for the replacement of utilities, sanitary and technological equipment (electric stoves, cooking boiler, refrigeration equipment). The project of improvement provides repair of a roof and installation of a gable roof on the building of a dining room. 

The design decision is made to perform works on replacement of window and door blocks, floor covering, internal finishing works, works on the equipment of household rooms in buildings; modernization of the heating system. 

Improvement project will involve the installation of ramps, elektropodemom equipment and antisplash coverings for wheelchair users.

Figure 2. The elements of the ramp
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Legend: 1 – march of the ramp; 2 – area in front of the ramp; 3 – intermediate; 4 – warning strip
4. Description of solutions to ensure the living conditions of people with limited mobility
It is necessary to provide conditions for unhindered and convenient movement of low-mobility groups on the territory of design, taking into account the requirements of town-planning norms to the parameters of the routes. Trace projected pedestrian paths-short, straight, visible throughout. Disabled Parking spaces are located in the immediate vicinity of the property.
The smallest width of the sidewalk is 1.5 m, the side stones are installed without a height difference, which ensures unhindered periodic movement of persons moving in wheelchairs from the driveways on the sidewalk to the sites located at the entrance to the building. The dimensions of the platforms allow to perform a free turn of the wheelchair both directly at the entrance to the building and along the path of wheelchair users.

The project provides for duplicate stairs, sidewalks-ramps for the disabled with a slope not exceeding 58 %. The longitudinal slope of the road, which is possible to travel disabled people in wheelchairs, adopted 0.5%-5.8%. At the device of exits from the sidewalk the longitudinal bias is increased to 10% at distance of 2.0 m from a Board road stone. Crossfall is adopted in the range of 1-25%.
Exits from the sidewalks to the roadway are made with a slope of 5-10%, the size of the site before the start of the Congress is 0.8-1.5 m, the color and texture throughout contrast with the color and texture of the adjacent surfaces.

The levels of crossing of the paths of motion on the sidewalk with driveways on one level. The height of the Board stone at the intersection of sidewalks with the roadway, as well as the curbs of the side stones along the operated lawns and landscaped areas adjacent to the paths of pedestrian traffic, are installed without a height difference.

To cover the pedestrian walkway, it is necessary to apply concrete paving slabs, small-piece. The surface of the coating is durable, hard, non-slip, the thickness of the seams between the tiles is not more than 10 mm, which provides unhindered and convenient movement of disabled groups on the footpath.

